Identifies the layer and bandwidth (rate) of the Topological Link.
The Layer Rate of a TL is determined by the lowest common Layer Rate of the two end point TPs, about which the EMS has knowledge (with the physical layer being the very lowest).

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
