This operation is used to query all currently applied TCA parameters on a PM Parameter within a PMP.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when any input parameter is syntactically incorrect.
3. ENTITY_NOT_FOUND - Raised when PMP does not exist.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.
