Configures all threshold values of a TCA Parameter Profile. This operation overwrites all the existing threshold values of the profile with the new provided threshold values.
Then all threshold values of all the TPs contained in the attribute associatedTPs within the TCAParameterProfile will be changed according to the new values.

The EMS has to return all TPs that could not be changed to the new threshold values due to some error reasons.

See corresponding activity diagram.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter are syntactical incorrect.
4. ENTITY_NOT_FOUND - Raised when TCA Parameter Profile to be changed does not exist.
5. NE_COMM_LOSS - Raised when communication to managed element is lost.
