The optional Specific Problems parameter, when present in an alarm notification, identifies further refinements to the Probable Cause of the alarm.
Note: It is similar to ProbableCauseQualifier, but this parameter is designed to be human readable and compatible with ITU usage.
This is consistent with the ITU-T X.733 definition.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
