Operation void getContainedInUseCTPNames (CIS SequenceOf Enums::LayerRate layerRateList = empty list, CIS SequenceOf Name ctpNames = NA), in Class TerminationPoint

Documentation
This operation is used to retrieve the names of the "in use" CTPs that are contained within a specific PTP or CTP, at specific layer rates. An "in use" CTP is defined as a CTP that is used by an SNC in any state (including pending), either as a CM end point or as an intermediate connection point, or a CTP that is terminated and mapped. This operation will be used when there are a large number of potential CTPs (e.g., in ATM).
Examples for contained InUse TPs in different states of usage are contained in the associated supporting document ContainedTPs.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when layerRateList contains undefined rates.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.
External Documents

SD1-6_ContainedTPs.pdf |

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

layerRateList
/* in */ The list of rates of the contained in use CTPs to be returned. An empty list indicates to the EMS to get all contained in use CTPs (for all rates).
ctpNames
/* out */ CTP object name(s) for any contained CTP(s).