Class TransmissionDescriptorCreateData {Analysis}

Documentation
Specifies the attributes required for the creation of a transmission descriptor. The NMS passes this to the EMS at TMD creation time.
Object Lifecycle: This is part of TMD creation request.
Object Creation Notification Issued? No
Object Deletion Notification Issued? No

Parent Package | Logical View | Abstract | No
Export Control | PublicAccess | Link Class for | None
Class Kind | NormalClass | Cardinality | n
Space |  | Concurrency | Sequential
Persistence | No |  |

Attributes

Name | Class | Type | Initial Value
userLabel | TransmissionDescriptorCreateData | CIS CharacterString | empty string
forceUniqueness | TransmissionDescriptorCreateData | CIS Boolean | TRUE
owner | TransmissionDescriptorCreateData | CIS CharacterString | empty string
additionalTPInfo | TransmissionDescriptorCreateData | CIS SequenceOf Structs::AVP | empty list
containingTMDName | TransmissionDescriptorCreateData | Name | CIS Null
externalRepresentationReference | TransmissionDescriptorCreateData | CIS CharacterString | empty string
additionalCreationInfo | TransmissionDescriptorCreateData | CIS SequenceOf Structs::AVP | empty list

Associations

Name | My Role | My Class | Other Role | Other Element
--Not Named-- | --Not Named-- | TransmissionDescriptorCreateData | transmissionParameters | TransmissionParameters