Operation void getAssociatedGroupTerminationPoint (GroupTerminationPoint returnedGTP = NA), in Class ConnectionTerminationPoint

Documentation
This operation returns the name of the GTP the CTP is associated to. If the CTP is not associated to a GTP, the returnedGTP parameter is left empty.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to managed element is lost and communication with
the managed element is needed to determine the GTP the CTP is associated to.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

returnedGTP
/* out */ Contains the name of the GTP the CTP is associated to.