Gets all threshold values of a TCA Parameter Profile.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter are syntactical incorrect.
4. ENTITY_NOT_FOUND - Raised when specified TCA Parameter Profile does not exist.
5. NE_COMM_LOSS - Raised when communication to managed element is lost.
