CIS SequenceOf Structs::AlarmSeverityAssignment alarmSeverityAssignmentList = empty list, in Class AlarmSeverityAssignmentProfile

Documentation
Each record of this sequence specifies the probable cause (plus optionally the probableCauseQualifier and / or the nativeProbableCause) and the severities to be assigned.
Changes in the value of this attribute lead to a AVC notification.
Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No

Export Control | PrivateAccess | Containment | Unspecified
Static | No | Derived | No