The optional Proposed Repair Actions parameter, when present in an alarm notification, is used if the cause is known and the system being managed can suggest one or more solutions (such as switch in standby equipment, retry, replace media).
This is consistent with the ITU-T X.733 definition.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
