tmf854.v1 > SwitchPosition_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The SwitchPosition_T Simple Type
This indicates whether the RING switch has occurred because of fault detection on this group or in a different group around the ring.
<ApplicableTo>2-F MSSPRING, 4-F MSSPRING</ApplicableTo>
Simple Type SwitchPosition_T
SwitchPosition_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (IDLE | PASS_THROUGH | SWITCH).

Enumeration | Description
IDLE |
PASS_THROUGH |
SWITCH |

XML
-<xsd:simpleType name="SwitchPosition_T"> -<xsd:annotation> -<xsd:documentation> This indicates whether the RING switch has occurred because of fault detection on this group or in a different group around the ring. <ApplicableTo>2-F MSSPRING, 4-F MSSPRING</ApplicableTo> </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="IDLE" /> <xsd:enumeration value="PASS_THROUGH" /> <xsd:enumeration value="SWITCH" /> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (1) PGPParameters_T/SwitchPosition

Generated by WSDLdoc ©