This attribute provides an indication of whether alarm reporting for this equipment holder is inhibited.TRUE allowed, FALSE inhibit.
Changes in the value of this attribute lead to an AVC notification.

Readable by NMS? Yes
Writeable by NMS? Yes
Invariant? No
