Get the name(s) of the containing subnetwork(s) of the Managed Element.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. COMM_LOSS - Raised when communication to managed element is lost.
