Operation void getContainedPotentialCTPNames (CIS SequenceOf Enums::LayerRate layerRateList = empty list, CIS SequenceOf Name ctpNames = NA), in Class TerminationPoint

Documentation
This operation is used to retrieve the names of the "potential" CTPs that are contained within a specific TP (PTP or CTP), at specific layer rates. Potential CTPs are all CTPs supported by all possible mapping configurations. If the layerRateList is empty then contained CTPs at all flexible and/or static LayerRates are returned.
Examples for contained Potential TPs in different states of usage are contained in the associated supporting document ContainedTPs.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2.INVALID_INPUT - Raised when layerRateList contains undefined rates.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.
External Documents

SD1-6_ContainedTPs.pdf |

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

layerRateList
/* in */ The list of rates of the contained potential CTPs to be returned. An empty list indicates to the EMS to get all contained potential CTPs (for all rates).
ctpNames
/* out */ CTP name(s) for any contained CTP(s).