This operation is used to discover all the equipment protection groups currently in
operation for the managed element.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure
3. NE_COMM_LOSS - Raised when communication to managed element is lost
