This operation activates alarm reporting on the topological link.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY -	Raised when alarm reporting can not be enabled.
