Operation void createTrafficDescriptor (TDCreateData newTDcreateData, TrafficDescriptor newTD), in Class EMS

Documentation
Creates a new Traffic Descriptor.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support creation of TDs via this interface.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when newTDCreateData contains invalid data.
4. USERLABEL_IN_USE - Raised when the userLabel uniqueness constraint is not met.
5. CAPACITY_EXCEEDED - Raised when maximum number of TDs has been reached.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
The TD has been established.
Semantics

Arguments

newTDcreateData
/* in */ The data that describes the traffic descriptor to create.
newTD
/* out */ The Traffic Descriptor distinguishing information.