This attribute defined the granularity of the performance monitoring measurement interval. For counters two values "15min" or "24h" are supported. For current instantaneous measurements the granularity does not apply which is indicated by the value "NA".

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
