This attribute describes dropping of a protection leg from the original SNC. Either the last cross-connects (that contain the SNCP) are specified by the NMS or the full route may be specified.This parameter can be used in conjonction with addedOrNewRoute only to reroute a segment.

Readable by NMS? No
Writeable by NMS? Yes
Invariant? Yes
