Identifies the equipment that was protected when the switch occurred. For a M:N group,
protectedE always identifies the worker equipment instance for which the switch occured.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
