This operation has exactly the same behaviour as getSupportingEquipment, but returns the object names instead of returning the entire objects.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to managed element is lost.
