The operation allows an NMS to request the intended route of the SNC.

Note: The relationship between Bundled SNC service and the SNC with Multiple Routes feature requires further study and is not applicable for v3.0.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when an EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY - Raised when the EMS is unable to execute the request because at least one of the
    parameters although valid can not be set and that parameter is identified as "not best effort" in additionalInfo.
    If the EMS cannot determine the reason it could not comply, it is also allowed to throw UNABLE_TO_COMPLY.
