Indicates the connectionState of the associated CTPs. All CTPs associated to a GTP shall have the same connectionState.
Changes in the value of this attribute lead to a State Change notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? No
