tmf854.v1 > SubnetworkConnection_T > rerouteAllowed
LOCATION: file:/xsd/networkResources/SubnetworkConnection.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The rerouteAllowed Element
This attribute indicates if the EMS/MEs are allowed and/or required to reroute this SNC if there is a failure on this SNC, periodically to optimize the routes, of for any other reason.It is an EMS/ME implementation whether this is done using network routing protocols or if the EMS/MEs detect the failure and take appropriate action to attempt to fix the SNC
Element SubnetworkConnection_T/rerouteAllowed : Reroute_T [0 .. 1]
The rerouteAllowed element can have "xsi:nil" as an attribute. The rerouteAllowed element in XML instance can be substituted with other elements.

XML Instance
This attribute indicates if the EMS/MEs are allowed and/or required to reroute this SNC if there is a failure on this SNC, periodically to optimize the routes, of for any other reason.It is an EMS/ME implementation whether this is done using network routing protocols or if the EMS/MEs detect the failure and take appropriate action to attempt to fix the SNC <rerouteAllowed>Reroute_T</rerouteAllowed>

﻿

Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes

﻿

XML
-<xsd:element minOccurs="0" name="rerouteAllowed" nillable="true" type="Reroute_T"> -<xsd:annotation> <xsd:documentation> This attribute indicates if the EMS/MEs are allowed and/or required to reroute this SNC if there is a failure on this SNC, periodically to optimize the routes, of for any other reason.It is an EMS/ME implementation whether this is done using network routing protocols or if the EMS/MEs detect the failure and take appropriate action to attempt to fix the SNC </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) Reroute_T

Used-By

Generated by WSDLdoc ©