Get a set of CTPs that are associated with the Traffic Descriptor.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to the ME is lost.
