tmf854.v1 > WtrTime_T LOCATION: file:/xsd/networkResources/PGPParameters.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The WtrTime_T Simple Type
This is the time required to wait before the revertive switch can go back to the primary TP. Values are in seconds or "-1" indicates an unknown value or that the parameter is not applicable.
<ApplicableTo>For revertive switches. 1+1 trail protection,1:N trail protection,2-F MSSPRING, 4-F MSSPRING</ApplicableTo>
Simple Type WtrTime_T
WtrTime_T is derived from integer type. There are several restrictions on the value. The range of the value is [-1..*]. The schema processor collapses value's whitespace. The number of fractional digits is less than or equals to 0.

XML
-<xsd:simpleType name="WtrTime_T"> -<xsd:annotation> -<xsd:documentation> This is the time required to wait before the revertive switch can go back to the primary TP. Values are in seconds or "-1" indicates an unknown value or that the parameter is not applicable. <ApplicableTo>For revertive switches. 1+1 trail protection,1:N trail protection,2-F MSSPRING, 4-F MSSPRING</ApplicableTo> </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:integer"> <xsd:minInclusive value="-1" /> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) integer

Used-By
Element (1) PGPParameters_T/WtrTime

Generated by WSDLdoc ©