This operation is used by the NMS to get the latest switch status on a SNCP.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when an EMS is unable to support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.
