This operation inhibits (deactivates, or turns off) alarm reporting on an instant of the Equipment class or its subclasses. Only alarms from the equipment (not TP alarms) are set off.

Note: If alarm monitoring is disabled, then alarm reporting is disabled even if Alarm Severity Assignment Profile would allow it.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY - Raised when alarm reporting can not be disabled.
4. NE_COMM_LOSS - Raised when communication to the managed element is lost.
