Get the Termination Point and its associated distinguishing information identified by an NMS-specified name.

Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. INVALID_INPUT - Raised when tpName does not reference a termination point object.
3. ENTITY_NOT_FOUND - Raised when tpName references a TP object that does not exist.
4. NE_COMM_LOSS - Raised when communication to managed element is lost.
