Defines if an original route of the SNC is maintained and that it is possible to swap back this route.
Changes in the value of this attribute lead to a AVC notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? No
