Indicates whether alarm reporting for the equipment is administratively activated or de-activated.

True = alarm reporting is activated; False = alarm reporting is de-activated.

Readable by NMS? No
Writeable by NMS? Yes
Invariant? Yes
