tmf854.v1 > ConnectionTerminationPoint_T > transmissionParams
LOCATION: file:/xsd/networkResources/TerminationPoint.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The transmissionParams Element
A list of transmission parameters which can be set and/or retrieved on the TP at a specified layer. This attribute must contain the complete set of layer rates represented by a PTP/CTP/FTP - even if they have no parameters associated with them. The layerRates are listed in the order of their client-server relationship (see layering for more details). This attribute can be set by an NMS through the managedElementManager :: ManagedElementMgr_I :: setTPData() operation and also during SNC creation. The values for the name field and the value fields of the NVSList_T are defined in Layered Parameters.
Element ConnectionTerminationPoint_T/transmissionParams : LayeredParametersList_T [0 .. 1]
The transmissionParams element can have "xsi:nil" as an attribute. The transmissionParams element in XML instance can be substituted with other elements.

XML Instance
A list of transmission parameters which can be set and/or retrieved on the TP at a specified layer. This attribute must contain the complete set of layer rates represented by a PTP/CTP/FTP - even if they have no parameters associated with them. The layerRates are listed in the order of their client-server relationship (see layering for more details). This attribute can be set by an NMS through the managedElementManager :: ManagedElementMgr_I :: setTPData() operation and also during SNC creation. The values for the name field and the value fields of the NVSList_T are defined in Layered Parameters. <transmissionParams> <layeredParameters extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T">LayeredParameters_T</layeredParameters> [0..*] </transmissionParams>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:element minOccurs="0" name="transmissionParams" nillable="true" type="LayeredParametersList_T"> -<xsd:annotation> <xsd:documentation> A list of transmission parameters which can be set and/or retrieved on the TP at a specified layer. This attribute must contain the complete set of layer rates represented by a PTP/CTP/FTP - even if they have no parameters associated with them. The layerRates are listed in the order of their client-server relationship (see layering for more details). This attribute can be set by an NMS through the managedElementManager :: ManagedElementMgr_I :: setTPData() operation and also during SNC creation. The values for the name field and the value fields of the NVSList_T are defined in Layered Parameters. </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) LayeredParametersList_T

Used-By

Generated by WSDLdoc ©