Operation void getSupportingEquipment (CIS SequenceOf Equipment equipmentList = empty list), in Class Equipment

Documentation
This operation allows an NMS to request all of the equipments that supports the equipment, e.g., the power pack and synchronization card that support a given piece of equipment.
Operation Exceptions:
1. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
2. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
No change in the system.
Semantics

Arguments

equipmentList
/* out */ Contains the list of equipments that support the equipment.