Identifies the total number of TPs or GTPs currently contained in the TPPool.
Changes in the value of this attribute lead to a AVC notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? No
