The optional Monitored Attributes parameter, when present in an alarm notification, defines one or more attributes of the managed object and their corresponding values at the time of the alarm.
This is consistent with the ITU-T X.733 definition.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
