Defines that not any other routes of other SNCs can share any of the routes XCs or CTPs, even in pending state (True).

Changes in the value of this attribute lead to a AVC notification.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes
