tmf854.v1 > getPotentialFixedCCs_T LOCATION: file:/xsd/interfaces/ManagedElementMgr.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The getPotentialFixedCCs_T Complex Type
The operation is used to retrieve fixed connection schemes related to normal and inverse multiplexing. See Subnetwork Connection Types for an explanation of fixed SNCs. The operation takes as an input a TP and if this TP may be or is involved in a multiplexing or inverse multiplexing scheme, it will report: - The TP containing the fixed layer. - the list of potential fixed cross connects that will exist if the containing TP's clientConnectivity or serverConnectivity is set to "Connected" (i.e. If the containing TP is set to multiplexing or inverse multiplexing). If the clientConnectivity (resp. serverConnectivity) of the TP is currently set to "Connected", the potentialCCList matches the list of active fixed cross connects that involve its client TPs (resp. server TPs). If the TP client layer (resp. server layer) is always fixed cross connected (hard-wired), the potentialCCList always matches the list of active fixed cross connects that involve the client TPs (resp. server TPs). Raises ProcessingFailureException EXCPT_NOT_IMPLEMENTED - Raised if the OS does not support this service EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised if inputTP does not reference a TP. EXCPT_ENTITY_NOT_FOUND - Raised when inputTP references a TP object that does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost EXCPT_UNABLE_TO_COMPLY - Raised when TP is neither a higher order TP that supports fixed multiplexing nor a lower order TP that supports fixed inverse multiplexing

Local elements (1)
  inputTP

Complex Type getPotentialFixedCCs_T
The getPotentialFixedCCs_T type does not allow mixed content. There is no restriction on type derivation.

XML Instance
<... extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T"> any TP name of the ME. The operation will return the multiplexing or inverse multiplexing scheme in which this TP is involved. The input TP may be either the containing TP or one of the end TPs of the portentialCCList. <inputTP extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</inputTP> [1..1] </...>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:complexType name="getPotentialFixedCCs_T"> -<xsd:annotation> <xsd:documentation> The operation is used to retrieve fixed connection schemes related to normal and inverse multiplexing. See Subnetwork Connection Types for an explanation of fixed SNCs. The operation takes as an input a TP and if this TP may be or is involved in a multiplexing or inverse multiplexing scheme, it will report: - The TP containing the fixed layer. - the list of potential fixed cross connects that will exist if the containing TP's clientConnectivity or serverConnectivity is set to "Connected" (i.e. If the containing TP is set to multiplexing or inverse multiplexing). If the clientConnectivity (resp. serverConnectivity) of the TP is currently set to "Connected", the potentialCCList matches the list of active fixed cross connects that involve its client TPs (resp. server TPs). If the TP client layer (resp. server layer) is always fixed cross connected (hard-wired), the potentialCCList always matches the list of active fixed cross connects that involve the client TPs (resp. server TPs). Raises ProcessingFailureException EXCPT_NOT_IMPLEMENTED - Raised if the OS does not support this service EXCPT_INTERNAL_ERROR - Raised in case of non-specific OS internal failure EXCPT_INVALID_INPUT - Raised if inputTP does not reference a TP. EXCPT_ENTITY_NOT_FOUND - Raised when inputTP references a TP object that does not exist EXCPT_COMM_FAILURE - Raised when communication to an entity (needed to help fulfill the request) is lost EXCPT_UNABLE_TO_COMPLY - Raised when TP is neither a higher order TP that supports fixed multiplexing nor a lower order TP that supports fixed inverse multiplexing </xsd:documentation> </xsd:annotation> -<xsd:sequence> -<xsd:element name="inputTP" type="NamingAttributes_T"> -<xsd:annotation> <xsd:documentation> any TP name of the ME. The operation will return the multiplexing or inverse multiplexing scheme in which this TP is involved. The input TP may be either the containing TP or one of the end TPs of the portentialCCList. </xsd:documentation> </xsd:annotation> </xsd:element> </xsd:sequence> <xsd:attribute name="extVersion" type="xsd:string" use="optional" /> <xsd:attribute name="extAuthor" type="xsd:string" use="optional" /> <xsd:attribute name="tmf854Version" type="TMF854_Version_T" use="optional" /> </xsd:complexType>

﻿

Uses
Type (3) NamingAttributes_T string TMF854_Version_T

Used-By
Element (1) getPotentialFixedCCs

Generated by WSDLdoc ©