This operation allows the NMS to know how many hours PM data records are held in the EMS (worst case time).

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.
