Integer CONTRA_FAR_END_RX = 4, in Class PMLocation

Documentation
Identifies a unidirectional measurement provided by a sink monitoring function that supervises the signal which is related to the source atomic function of this TP. The opposite direction of the supervised signal is measured.
See attached document for clarification.
Readable by NMS? Yes
Writeable by NMS? No
Invariant? Yes

Export Control | PublicAccess | Containment | Unspecified
Static | No | Derived | No