tmf854.v1 > Reroute_T LOCATION: file:/xsd/networkResources/SubnetworkConnection.xsd
SECTIONS: Basic | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The Reroute_T Simple Type
The Reroute_T type indicates if the EMS/MEs are allowed and/or required to reroute this SNC if there is a failure on this SNC, periodically to optimize the routes, of for any other reason.It is an EMS/ME implementation whether this is done using network routing protocols or if the EMS/MEs detect the failure and take appropriate action to attempt to fix the SNC. The RR_NO value means that the EMS/MEs are not allowed to reroute the SNC. The RR_YES value means that the EMS/MEs are allowed to reroute the SNC and required to attempt to reroute it upon failure. The RR_NA value is used when the NMS does not want to specify the exact EMS behaviour. In this case it is left up to the EMS to decide whether rerouting will be provided. It is also used if the EMS/MEs are allowed to reroute the SNC but not required to attempt to reroute it upon failure.
Simple Type Reroute_T
Reroute_T is derived from string type. There are several restrictions on the value. The schema processor preserves value's whitespace. Enumeration values are (RR_NA | RR_NO | RR_YES).

Enumeration | Description
RR_NA |
RR_NO |
RR_YES |

XML
-<xsd:simpleType name="Reroute_T"> -<xsd:annotation> <xsd:documentation> The Reroute_T type indicates if the EMS/MEs are allowed and/or required to reroute this SNC if there is a failure on this SNC, periodically to optimize the routes, of for any other reason.It is an EMS/ME implementation whether this is done using network routing protocols or if the EMS/MEs detect the failure and take appropriate action to attempt to fix the SNC. The RR_NO value means that the EMS/MEs are not allowed to reroute the SNC. The RR_YES value means that the EMS/MEs are allowed to reroute the SNC and required to attempt to reroute it upon failure. The RR_NA value is used when the NMS does not want to specify the exact EMS behaviour. In this case it is left up to the EMS to decide whether rerouting will be provided. It is also used if the EMS/MEs are allowed to reroute the SNC but not required to attempt to reroute it upon failure. </xsd:documentation> </xsd:annotation> -<xsd:restriction base="xsd:string"> <xsd:enumeration value="RR_NA" /> <xsd:enumeration value="RR_NO" /> <xsd:enumeration value="RR_YES" /> </xsd:restriction> </xsd:simpleType>

﻿

Uses
Type (1) string

Used-By
Element (1) SubnetworkConnection_T/rerouteAllowed

Generated by WSDLdoc ©