Operation void createTCAParameterProfile (Name managedElementName = NA, LayerRate layerRate = NA, CIS SequenceOf TCAParameter listOfTCAParameter = NA, CIS CharacterString userLabel = empty string, Boolean forceUniqueness = True, CIS CharacterString owner = empty string, CIS SequenceOf Structs::AVP additionalInfo = empty list, TCAParameterProfile tcaParameterProfile = NA), in Class PerformanceManager

Documentation
Creates a new TCA Parameter Profile.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when input parameter are syntactical incorrect.
4. ENTITY_NOT_FOUND - Raised when specified managed element does not exist.
5. USERLABEL_IN_USE - Raised when the userLabel uniqueness constraint is not met.
6. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
New TCA Parameter Profile is created, containing the requested threshold values.
Semantics

Arguments

managedElementName
/* in */ ME under which the profile is to be created.
layerRate
/* in */ Defines the layer rate of the profile to be created.
listOfTCAParameter
/* in */ The listOfTCAParameter parameter contains sets of threshold values.
userLabel
/* in */ The userLabel parameter contains the NMS defined name of the profile to be created.
forceUniqueness
/* in */ If set to TRUE the EMS has to check if the provided user label is unique
in the network element domain.
owner
/* in */ A label of the owner of the Profile. This is an optional parameter.
additionalInfo
/* in */ Some additional information may be specified by the NMS.
tcaParameterProfile
/* out */ The EMS will return the new profile to the NMS.