tmf854.v1 > Alarm_T > affectedTPList
LOCATION: file:/xsd/networkResources/Notifications.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The affectedTPList Element
A list of affected TPs. Contained CTPs are not listed. This field is optional for all alarms except for alarms on equipment. This is used to indicate a list of TPs affected by an equipment failure for example. If the alarm is an alarm on an equipment that supports PTPs, then the ports (PTPs) supported by this equipment will be listed in this field (irrespective of whether the alarm is Service Affecting or not). The list should be ordered by PTP names (ASCII order).
Element Alarm_T/affectedTPList : NamingAttributesList_T [0 .. 1]
The affectedTPList element cannot have "xsi:nil" as an attribute. The affectedTPList element in XML instance can be substituted with other elements.

XML Instance
A list of affected TPs. Contained CTPs are not listed. This field is optional for all alarms except for alarms on equipment. This is used to indicate a list of TPs affected by an equipment failure for example. If the alarm is an alarm on an equipment that supports PTPs, then the ports (PTPs) supported by this equipment will be listed in this field (irrespective of whether the alarm is Service Affecting or not). The list should be ordered by PTP names (ASCII order). <affectedTPList extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T"> <name extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</name> [0..*] </affectedTPList>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:element minOccurs="0" name="affectedTPList" type="NamingAttributesList_T"> -<xsd:annotation> <xsd:documentation> A list of affected TPs. Contained CTPs are not listed. This field is optional for all alarms except for alarms on equipment. This is used to indicate a list of TPs affected by an equipment failure for example. If the alarm is an alarm on an equipment that supports PTPs, then the ports (PTPs) supported by this equipment will be listed in this field (irrespective of whether the alarm is Service Affecting or not). The list should be ordered by PTP names (ASCII order). </xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) NamingAttributesList_T

Used-By

Generated by WSDLdoc ©