This operation allows (activates, or turns on) alarm reporting on this equipment holder.

Note: If alarm monitoring is enabled, this does not mean that alarm is reported anyway, because Alarm Severity Assignment Profile may perform further filtering.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. UNABLE_TO_COMPLY -	Raised when alarm reporting can not be enabled.
4. NE_COMM_LOSS - Raised when communication to the managed element is lost.
