This operation allows the NMS to request a filtered set (scoped by the input parameter pmParameters) history PM data for a list of TP measurement points. The requested data will be returned immediately instead of file. This is a complimentary to file based retrieval used in the operation getHistoryPMData.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when any input parameter is syntactically incorrect.
4. ENTITY_NOT_FOUND - Raised when pmTPSelectList refer to an object that does not exist.
5. UNABLE_TO_COMPLY - Raised when EMS does not support history PM for the time period specified by NMS.
6. NE_COMM_LOSS - Raised when communication to managed element is lost.
