Operation void retrieveESwitchData (CIS SequenceOf ESwitchData eSwitchDataList), in Class EquipmentProtectionGroup

Documentation
This operation is used to get the latest switch status on an equipment protection group.
For a retrieval of a revertive M:N group, N ESwitchData objects are returned (one for each
worker equipment instance).
For a retrieval of a non-revertive M:N group, N ESwitchData objects are returned (one for
each active equipment instance).
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS does not support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
The switch data is available to the NMS.
Semantics

Arguments

eSwitchDataList
/* out */ The current protection switch status of the equipment protection group.