Operation void setTCAParameter (CIS SequenceOf PerformanceMonitoringPoint pmps = NA), in Class TerminationPoint

Documentation
This operation is used to set TCA parameters on a TP.
Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when the EMS is unable to support this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. INVALID_INPUT - Raised when at least one field of tcaParameters is not valid.
4. ENTITY_NOT_FOUND - Raised when any PMP to be set does not exist.
5. NE_COMM_LOSS - Raised when communication to managed element is lost.

Protocol |  | Qualification |
Exceptions |  | Size |
Time |  | Concurrency | Sequential
Export Control | PublicAccess |  |

Preconditions
None
Postconditions
TCA thresholds are modified on the TP.
Semantics

Arguments

pmps
/* in */ The list of PMPs to be set.