tmf854.v1 > getAllUnacknowledgedActiveAlarmsResponse_T > activeAlarmList > activeAlarm
LOCATION: file:/xsd/interfaces/ManagedElementMgr.xsd
SECTIONS: Basic | XML Instance | Attributes | XML | Reference Overview | TOC | No TOC | Help
tmf854.v1
The activeAlarm Element
An Active alarm
Element getAllUnacknowledgedActiveAlarmsResponse_T/activeAlarmList/activeAlarm : Alarm_T [1 .. *]
The activeAlarm element cannot have "xsi:nil" as an attribute. The activeAlarm element in XML instance can be substituted with other elements.

XML Instance
An Active alarm <activeAlarm> -Begin All [1...1] The set of event information attributes. <eventInfo>EventInformation_T</eventInfo> [1..1] Indicates if the event is clearable (or is itself a clear). <isClearable>xsd:boolean</isClearable> [1..1] Identifies all the object list of aliases to describe the network entity as portrayed on the OS user interface. <aliasNameList extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">AliasNameList_T</aliasNameList> [0..1] The layer which this alarm is relevant to. <layerRate>LayerRate_T</layerRate> [1..1] No other string than the ones defined by the TM Forum should be used for this field. <probableCause overlap="xsd:string" qualifier="xsd:string">ProbableCause_T</probableCause> [1..1] Identifies the probableCause as portrayed on the OS user interface. <nativeProbableCause>xsd:string</nativeProbableCause> [0..1] More information about the alarm. such as, "Unit is mismounted". <additionalText>xsd:string</additionalText> [0..1] Indicates the severity of the alarm. <perceivedSeverity>PerceivedSeverity_T</perceivedSeverity> [1..1] A list of affected TPs. Contained CTPs are not listed. This field is optional for all alarms except for alarms on equipment. This is used to indicate a list of TPs affected by an equipment failure for example. If the alarm is an alarm on an equipment that supports PTPs, then the ports (PTPs) supported by this equipment will be listed in this field (irrespective of whether the alarm is Service Affecting or not). The list should be ordered by PTP names (ASCII order). <affectedTPList extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributesList_T</affectedTPList> [0..1] Indicates whether the alarm has affected service <serviceAffecting>ServiceAffecting_T</serviceAffecting> [1..1] The RCAI indicator has two values, i.e., TRUE (meaning that the alarm is a Root Cause Alarm Indication) or FALSE (meaning the alarm is a raw alarm). <rcaiIndicator>xsd:boolean</rcaiIndicator> [1..1] The acknowledge indication state. <acknowledgeIndication>AcknowledgeIndication_T</acknowledgeIndication> [0..1] Classifies the alarm into one of the five basic categories specified in ITU-T X.733. Value is one of the following: "communicationsAlarm", "environmentalAlarm", "equipmentAlarm", "processingErrorAlarm", "qualityofServiceAlarm" This field is optional. <X733_EventType>xsd:string</X733_EventType> [0..1] Identifies further refinements to the Probable cause of the alarm. (Similar to ProbableCauseQualifier, but this parameter is designed to be human readable and compatible with ITU usage.) This field is optional. <X733_SpecificProblems>SpecificProblemList_T</X733_SpecificProblems> [0..1] Specifies whether or not the object emitting the alarm has been backed-up, and services provided to the user have, therefore, not been disrupted. Value is one of the following: "BACKED_UP", "NOT_BACKED_UP" This field is optional. <X733_BackedUpStatus>xsd:string</X733_BackedUpStatus> [0..1] Specifies the object that is providing back-up services for the object about which the notification pertains. This parameter shall be present when the X733::BackedupStatus parameter is present and has the value "BACKED_UP". This field is optional otherwise. <X733_BackUpObject extVersion="xsd:string" extAuthor="xsd:string" tmf854Version="TMF854_Version_T">NamingAttributes_T</X733_BackUpObject> [0..1] Specifies the current severity trend of the object. If present it indicates that there are one or more alarms ("outstanding alarms") which have not been cleared, and pertain to the same object as that to which this alarm ("current alarm") pertains. Value is one of the following: "MORE_SEVERE", "NO_CHANGE", "LESS_SEVERE" This field is optional. <X733_TrendIndication>xsd:string</X733_TrendIndication> [0..1] Contains a set of Notification identifiers and, if necessary, their associated object names. This set is defined to be the set of all notifications to which this notification is considered to be correlated. This field is optional. <X733_CorrelatedNotifications>CorrelatedNotificationList_T</X733_CorrelatedNotifications> [0..1] Defines one or more attributes of the managed object and their corresponding values at the time of the alarm. This field is optional. <X733_MonitoredAttributes>AnyList_T</X733_MonitoredAttributes> [0..1] Used if the cause is known and the system being managed can suggest one or more solutions (such as switch in standby equipment, retry, replace media). This field is optional. <X733_ProposedRepairActions>ProposedRepairActionList_T</X733_ProposedRepairActions> [0..1] The specific containment for vendor extensions of the Alarm notification object. <vendorExtensions extAuthor="xsd:string" extVersion="xsd:string" tmf854Version="TMF854_Version_T">AlarmExt_T</vendorExtensions> [0..1] End All </activeAlarm>

﻿

Attributes |
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
overlap | string | This attribute is optional. Its form is unqualified. Show details.
Base type of overlap is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
qualifier | string | This attribute is optional. Its form is unqualified. Show details.
Base type of qualifier is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
No Attributes
﻿
Name | Type | Summary
--- | --- | ---
extAuthor | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extAuthor is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
extVersion | string | This attribute is optional. Its form is unqualified. Show details.
Base type of extVersion is string. There are several restrictions on the value. The schema processor preserves value's whitespace.
tmf854Version | TMF854_Version_T | This attribute is optional. Its form is unqualified. Show details.
Base type of tmf854Version is string. There are several restrictions on the value. The schema processor preserves value's whitespace. The value must match "`1\.([0-9]|[A-Z]|[a-z])*`".

﻿

XML
-<xsd:element maxOccurs="unbounded" name="activeAlarm" type="Alarm_T"> -<xsd:annotation> <xsd:documentation>An Active alarm</xsd:documentation> </xsd:annotation> </xsd:element>

﻿

Uses
Type (1) Alarm_T

Used-By

Generated by WSDLdoc ©