This operation allows an NMS to request all of the active alarms and TCAs of the EMS System. These alarms only apply to the EMS platform.
Note: A raised alarm is called active as long as no clear notification was received.
Alarms which ASAP assigned severity is "NOT_ALARMED" should not be reported by this operation.

Operation Exceptions:
INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
