Indicates if the CTP is configured such that it is capable of supporting lower or higher rate connections or is capable of supporting connections at the CTP's layer rate.
Changes in the value of this attribute lead to a AVC notification.

Within the façade definition, the CTP/FTP can act as an aggregate of associated G.805 TCPs, G.805 Termination Functions and G.805 CPs at one or more LayerRates. The CTP is contained within a PTP or FTP. The tpMappingMode attribute indicates and controls the connection of the named CP at a specified LayerRate to the dedicated G.805 TCP and associated G.805 Termination Function at the same LayerRate within the CTP/FTP.

Readable by NMS? Yes
Writeable by NMS? No
Invariant? No
