This operation implements the relationship between a PTP and its zero, one or two ProtectionGroups.

Operation Exceptions:
1. NOT_IMPLEMENTED - Raised when EMS dos not supported this operation.
2. INTERNAL_ERROR - Raised in case of non-specific EMS internal failure.
3. NE_COMM_LOSS - Raised when communication to managed element is lost.
